Sporecollector1.py  
  
Address the sporecollector   
Supply 12 V with min 3 amp   
two options available to choose  
24V or 12 V pump  
we are using 24 V pump

Amount of liters to be sucked can be changed by assigning desired amount of liters to be sucked to variable z